Havant HWRC Fire boom deployment



In the unlikely event of a fire at the HWRC the primary containment method to prevent fire from spreading on site is to drag the container on fire into the centre of the HGV yard using RoRo vehicle or grab plant.

Once the container has been isolated a mobile fire boom can be deployed around the container allowing for any fire to be tackled and the firewater to be contained within the boom. The fire water can then be emptied by a road tanker, the surface cleaned and the bund removed. 

Further drain mats and absorbent booms will be placed to prevent secondary runoff from the isolated container.
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